Two scaled version of the watch: (x3.5 and x5.8)
Each file contains main and auxilary components.

Main parts:
face.stp
lever.stp
plate.stp
+ physical properties of each

Others:
other parts that are required to be assembled.
