Crate testing

Label crates - C1, C2, C3, (..) and note type / manuf
		Label front, top left
Label ventilation - V1, V2, V3, (..) and note type / manuf
		Label front, bottom left
Label power - P1, P2, P3 and note type / manuf
		Label where power cord emerges

Testing procedure
Assemble crate to be tested (power supply, crate, ventilation if there). Insert test load module. Test positive / negative, 



Crates

C1 		P1 		(no V)  fully operational
						looks like integrated power supply (no brand) 
C2 		P2 		V1 		fully operational
						Power supply 	Canberra 7530 #601/263
C3 
				V2 		(tested with C2, P2) - left and center fan broken 
				V3 		(tested with C2, P2) - noisy, right fan broken
C4 		P3 		(no V) 	SEN 350N3 
						(cooling through bottom, single PS fan)
						Seems fully operational under load, but ALARM light on right side of module comes on for all voltages? 
C5 		P4 		V4		Ventilation fully operational
						Crate fully operational
C6		P5		V5		Crate			Canberra 7507B
						Power supply 	Sekotronic 7530 #601/349
										+/-6V/15A, +/-12V/3A, +/-24V/3A, 300W (117V~/0.5A) 
						Ventilation fully operational
						Crate fully operational
C7 		P6 		V6		Power supply 		SEN PS2077 #036
						Crate gives alarm when loading down 6V
						

