Control checklist for biosafety level 2 laboratory (BSL 2) 
(Adapted from annex 2 of the Directive concerning the internal procedure for projects subject to notification/authorization according to the ContainO, RO and OPTM Ordinances » 

	BSL 2 laboratory and OHS-PR Biosafety control 

	OHS-PR Biosafety person
	

	Date of the audit 
	

	BSL 2 room number
	

	Name of the Unit
	

	BSO 
	



	WORK ORGANISATION

	BSL 2 Training courses
☐ yes	
☐ no
☐ partially
	

	Biosafety officer (BSO) training
☐ Continuing education in biosafety done recently
☐ No recent biosafety training
	

	Other visitors: 
☐ yes	
☐ no
☐ partially
		

	Written work instructions provided to users either electronically or on paper or displayed in the laboratory. 
Which format?
☐ yes	
☐ no
☐ partially
	

	Organism inventory 
Which format
☐ yes	
☐ no
☐ partially
	

	Organisms – information for every user and access to the organism sheets (if there are)
☐ yes	
☐ no
☐ partially
	

	Management of organism’s storage
How?
☐ storage in the lab
☐ storage out of the lab :
· Storage plan,
· Biohazard sign, 
· User list,
· « keep-out » sign
	

	Unit-specific biosafety concept 
☐ yes	
☐ no
☐ partially
	




	INFRASTRUCTURES

	Access control via CAMIPRO
☐ yes		
☐ no		 
N° Demande de travaux : 
	

	« Biohazard » sign:
☐ yes		
☐ no	

	

	« Keep-out » sign :
☐ yes		
☐ no	
	

	Door safety sheet :
· Up to date
· Representative examples of organisms mentioned
☐ yes		
☐ no	
	

	Air pressure on premises:
Not authorised to be in positive pressure in relation to adjoining corridor
☐ Positive pressure
☐ Atmospheric pressure
☐ Negative pressure
	

	Sealed windows :
NB: ContainO and ATCC regulation. If windows cannot be sealed, they must be closed while work is being carried out in P2 zone
☐ yes		
☐ no	
	

	Autoclave in the building with maintenance procedure
☐ yes		
☐ no
	

	Outside the SV faculty:
Autoclave in the building with filter to avoid potentially contaminated air being discharged into the room / water. (2 autoclaves in CH: LEAGO et EML + 1 in GR Tamar Kohn (LEV) + 2 in MXD PBL et LP)
☐ yes		
☐ no
	

	Outside the SV faculty:
Autoclave with ISO 17665 tests performed each 5 years
☐ yes		
☐ no
	

	Floor that can be easily cleaned with a disinfectant
☐ yes		
☐ no	
	

	Bench resistant to chemicals:
Water, acids, bases solvents, disinfectants, decontaminants
☐ yes		
☐ no	
	

	Order and cleanliness 
☐ yes		
☐ no	
	

	Floor drain present in the BSL 2 laboratory
☐ yes		
☐ no
		

	Items that can absorb and retain aerosols present in the laboratory (such as a CD player, etc.)
☐ yes		
☐ no	
	



	
EQUIPMENT & SAFETY EQUIPMENT

	Fix phone in the room
☐ yes		
☐ no		 
N° Demande d’intervention : 
	

	Biosafety cabinet
· with maintenance procedure
(BSC Class II for human pathogen manipulation)
☐ BSC class I
☐ BSC class II
☐ BSC class III
☐ None
Check completed on:
	 

	Aspiration system (for biosafety cabinets) such as the VACUSAFE
Filters are replaced regularly and the type of hydrophobic filter used is appropriate for the application (0.2 µm filters when handling viruses or viral vectors)
☐ yes		
☐ no
	

	Liquid waste treatment
How?
☐ yes		
☐ no	
	

	Rotors and « buckets » with safety lids
All buckets or rotors for centrifugation must be used with their safety lids. If the tubes were closed during centrifugation and no problems were experienced during the process, it is not necessary to transport the buckets and rotors under a hood to open them.
☐ yes		
☐ no		 
	

	Pipets and pipet-tips with aerosol protection
☐ yes		
☐ no	
		 

	Solid waste management
How? 
☐ yes		
☐ no	
☐ partially	 
	

	Waste transport to the autoclave room
☐ adapted
☐ non-adapted
	

	Eye-wash station
☐ yes		
☐ no	
		 	

	Decontamination and cleaning equipment
Which?
 ☐ yes		
☐ no	
WARNING: Biocidal is not effective against non-enveloped viruses
		 


	Cleaning management:
· organized (what, when, by who)
· tracked (log sheet, logbook, or other)
☐ yes		
☐ no		 
☐ partially
	

	Transport of samples between labs in the building or on campus
☐ adapted
☐ non-adapted
	



	PERSONAL PROTECTIVE EQUIPMENT

	Cotton lab coat or surgical gown with long sleeves and tight cuffs and procedure to clean and autoclave them
☐ yes		
☐ no	
☐ partially
	 

	Respiratory protection
NB: For activities during which use of a BSC is not possible, it may be requested that a mask is worn, e.g. stereotaxic injections.
☐ yes		
☐ no	
Reason:
	 

	Safety glasses or face mask
☐ yes		
☐ no	
Raison:
	 

	Gloves (EN 374/2 et EN 374/3)
☐ yes		
☐ no	

	

	Hand disinfectant:
Which?
☐ yes		
☐ no	
	

	Cover shoes or sticky mat at the entrance
☐ yes		
☐ no	
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