Bill of Material for 
On 01/11/2012 at 15:32:15

 Comment             Pattern     Quantity  Components
------------------------------------------------------------------------------
 (not fit)           CAPC1608N        1    C22                          Capacitor (Semiconductor SIM Model) 
 100                 RESC1608N        5    R30, R35, R37, R38, R39      Resistor             
 100n                CAPC1608N        2    C10, C31                     Capacitor (Semiconductor SIM Model) 
 100nF               CAPC1608N       11    C1, C2, C4, C5, C11, C18, C35 Capacitor (Semiconductor SIM Model) 
                                           C36, C37, C38, C39
 10K                 RESC1608N        6    R20, R28, R29, R31, R34, R36 Resistor             
 10n                 CAPC1608N        1    C28                          Capacitor (Semiconductor SIM Model) 
 10nH                INDC1608N        1    L2                           Inductor             
 10uH                WE-PD2-S         1    L1                           SELF_WE_PD2          
 12nH                INDC1608N        2    L3, L4                       Inductor             
 150R                RESC1608N        6    R1, R5, R18, R23, R24, R25   Resistor             
 1K                  RESC1608N        5    R2, R3, R4, R10, R32         Resistor             
 1M                  RESC1608N        1    R21                          Resistor             
 1nF                 CAPC1608N        2    C3, C6                       Capacitor (Semiconductor SIM Model) 
 1u                  CAPC1608N        2    C12, C19                     Capacitor (Semiconductor SIM Model) 
 1uF                 CAPC1608N        2    C8, C14                      Capacitor (Semiconductor SIM Model) 
 220nF               CAPC1608N        1    C15                          Capacitor (Semiconductor SIM Model) 
 220u 4V             CAP_SMD_B        1    C7                           Polarized Capacitor (Axial) 
 22K (1%)            RESC1608N        1    R22                          Resistor             
 22p                 CAPC1608N        3    C20, C30, C32                Capacitor (Semiconductor SIM Model) 
 22pF                CAPC1608N        2    C27, C29                     Capacitor (Semiconductor SIM Model) 
 22uF,35V            CAP_SMD_D        1    C13                          Polarized Capacitor (Surface Mount) 
 22uF,6.3V           CAP_SMD_A        1    C17                          PANASONIC EEFCD1B220 
 25m                 RESC1608N        1    R7                           Resistor             
 300R                RESC1608N        1    R8                           Resistor             
 330nF               CAPC1608N        1    C16                          Capacitor (Semiconductor SIM Model) 
 33K                 RESC1608N        1    R11                          Resistor             
 33p                 CAPC1608N        1    C26                          Capacitor (Semiconductor SIM Model) 
 3K3                 RESC1608N        2    R16, R17                     Resistor             
 3n3                 CAPC1608N        1    C24                          Capacitor (Semiconductor SIM Model) 
 4.7K                RESC1608N        2    R26, R27                     Resistor             
 47K                 RESC1608N        6    R12, R13, R14, R15, R19, R33 Resistor             
 4K7                 RESC1608N        1    R6                           Resistor             
 4p7                 CAPC1608N        1    C23                          Capacitor (Semiconductor SIM Model) 
 4u7                 CAPC1608N        1    C9                           Capacitor (Semiconductor SIM Model) 
 5p6                 CAPC1608N        2    C21, C25                     Capacitor (Semiconductor SIM Model) 
 8K2                 RESC1608N        1    R9                           Resistor             
 Battery             MM4              1    J1                           Header, 4-Pin        
 BSS138              SOT95P240-3M     1    Q3                           N-Channel Enhancement Mode Vertical DMOS FET 
 Buzzer              ABSM-1574        1    LS1                          Magnetic Transducer Buzzer 
 Cap                 CAPC1608N        2    C33, C34                     Capacitor            
 COAX-M              CONN_SMA         1    P3                           RF Coaxial PCB Connector, MMCX; Thru-Hole, Vertical Mount Plug,  50 Ohm Impedance 
 Component_1         PCBComponent_1    1    *1                                                
 D Schottky          DSO-C2/X2.3      2    D1, D2                       Schottky Diode       
 D Zener             SOD123           1    D7                           Zener Diode          
 DS2764              TSSOP16          1    U1                                                
 Header 10           HDR1X10          2    P8, P9                       Header, 10-Pin       
 Header 10X2         HDR2X10          1    P7                           Header, 10-Pin, Dual row 
 Header 3            HDR1X3           2    P10, P11                     Header, 3-Pin        
 Joystick1           HDR1X5           1    P1                           Header, 5-Pin        
 Joystick2           HDR1X5           1    P2                           Header, 5-Pin        
 LCD                 MM6              1    J3                           Header, 6-Pin        
 LED2                3.2X1.6X1.1      1    D8                           Typical RED, GREEN, YELLOW, AMBER GaAs LED 
 LT1571-5            TSOP65P640-16AN    1    U3                           Constant-Current/Constant-Voltage Battery Charger with Preset Voltage and Termination Flag 
 ltc3240             DFN6-DC          1    U2                           Step-Up/Step-Down Charge Pump DC/DC Converter 
 MCL4148             PCBComponent_1 - duplicate1    1    D3                           Default Diode        
 MM4                 MM4              1    P6                           Header, 4-Pin        
 MM4-IMU             MM4              1    P5                           Header, 4-Pin        
 MM6                 MM6              1    J4                           Header, 6-Pin        
 NRF905              QFN32_M          1    U5                           Single chip radio transceiver 
 Orange              0603_D           1    D5                                                
 PIC16LF876A-I/ML    QFN-ML28_M       1    U4                           Enhanced FLASH Microcontroller, 8K (x14-Bit words) FLASH, 368 Bytes RAM, 28-Pin QFN, Standard VDD Range, Industrial Temperature 
 PWRJACK             RASM712          1    J2                           Power Jack           
 Rouge               0603_D           1    D4                                                
 SD Slot             CONN_SD_3M       1    P4                           SD/MMC Card Connector 
 Si2315BDS           SOT23            2    Q1, Q2                       P-Channel Enhancement Mode Vertical DMOS FET 
 STM32F103CBT6       LQFP48_N         1    U6                           STM32 ARM-based 32-bit MCU with 128 Kbytes Flash, 48-pin LQFP, Industrial Temperature 
 SW-ON/OFF           JUMP2            1    S1                           Single-Pole, Single-Throw Switch 
 SW-PB               BTN_JPM1990-0101    5    S2, S3, S4, S5, S7           Switch               
 Vert                0603_D           1    D6                                                
 XTAL 8MHz           HC49/4H_SMX      1    Y3                           Crystal Oscillator   
 XTALGND             SX-7050          2    Y1, Y2                       Crystal Oscillator with ground 
