M-File Help: tr2angvec | View code for tr2angvec

# tr2angvec

Convert rotation matrix to angle-vector form

[theta,v] = tr2angvec(R, options) is rotation expressed in terms of an angle theta (1x1) about the axis v (1x3) equivalent to the orthonormal rotation matrix R (3x3).

[theta,v] = tr2angvec(T, options) as above but uses the rotational part of the homogeneous transform T (4x4).

If R (3x3xK) or T (4x4xK) represent a sequence then theta (Kx1)is a vector of angles for corresponding elements of the sequence and v (Kx3) are the corresponding axes, one per row.

## Options

'deg' | Return angle in degrees

## Notes

- If no output arguments are specified the result is displayed.

## See also

angvec2r, angvec2tr

© 1990-2014 Peter Corke.