M-File Help: CodeGenerator | View code for CodeGenerator

# CodeGenerator

Class for code generation

Objects of the CodeGenerator class automatcally generate robot specific code, as either M-functions, C-functions, C-MEX functions, or real-time capable Simulink blocks.

The various methods return symbolic expressions for robot kinematic and dynamic functions, and optionally support side effects such as:

- M-functions with symbolic robot specific model code
- real-time capable robot specific Simulink blocks
- mat-files with symbolic robot specific model expressions
- C-functions and -headers with symbolic robot specific model code
- robot specific MEX functions based on the generated C-code (C-compiler must be installed).

## Example

    % load robot model
    mdl_twolink

    cg = CodeGenerator(twolink);
    cg.geneverything();

    % a new class has been automatically generated in the robot directory.
    addpath robot

    tl = @robot();
    % this class is a subclass of SerialLink, and thus polymorphic with
    % SerialLink but its methods have been overloaded with robot-specific code,
    % for example
    T = tl.fkine([0.2 0.3]);
    % uses concise symbolic expressions rather than the generalized A-matrix
    % approach

    % The Simulink block library containing robot-specific blocks can be
    % opened by
    open robot/robotslib.slx
    % and the blocks dragged into your own models.

## Methods

gencoriolis | generate Coriolis/centripetal code
genfdyn | generate forward dynamics code
genfkine | generate forward kinematics code
genfriction | generate joint friction code
gengravload | generate gravity load code
geninertia | generate inertia matrix code
geninvdyn | generate inverse dynamics code
genjacobian | generate Jacobian code
geneverything | generate code for all of the above

## Properties (read/write)

basepath | basic working directory of the code generator
robjpath | subdirectory for specialized MATLAB functions
sympath | subdirectory for symbolic expressions
slib | filename of the Simulink library
slibpath | subdirectory for the Simulink library
verbose | print code generation progress on console (logical)
saveresult | save symbolic expressions to .mat-files (logical)
logfile | print modeling progress to specified text file (string)
genmfun | generate executable M-functions (logical)
genslblock | generate Embedded MATLAB Function blocks (logical)
genccode | generate C-functions and -headers (logical)
genmex | generate MEX-functions as replacement for M-functions (logical)
compilemex | automatically compile MEX-functions after generation (logical)

## Properties (read only)

rob | SerialLink object to generate code for (1x1).

## Notes

- Requires the MATLAB Symbolic Toolbox.
- For robots with > 3 joints the symbolic expressions are massively complex, they are slow and you may run out of memory.
- As much as possible the symbolic calculations are down row-wise to reduce the computation/memory burden.
- Requires a C-compiler if robot specific MEX-functions shall be generated as m-functions replacement (see MATLAB documentation of MEX files).

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

SerialLink, Link

# CodeGenerator.CodeGenerator

Construct a code generator object

cGen = CodeGenerator(rob, options) is a code generator object for the SerialLink object rob.

## Options

CodeGenerator has many options, and useful sets of options are called optionSets, and the following are recognized:

'default' | set the options: verbose, saveResult, genMFun, genSLBlock
'debug' | set the options: verbose, saveResult, genMFun, genSLBlock and create a logfile named 'robModel.log' in the working directory
'silent' | set the options: saveResult, genMFun, genSLBlock
'disk' | set the options: verbose, saveResult
'workspace' | set the option: verbose; just outputs symbolic expressions to workspace
'mfun' | set the options: verbose, saveResult, genMFun
'slblock' | set the options: verbose, saveResult, genSLBlock
'ccode' | set the options: verbose, saveResult, genCcode
'mex' | set the options: verbose, saveResult, genMEX

If no optionSet is provided, then 'default' is used.

The options themselves control the code generation and user information:

'verbose' | write code generation progress to command window
'saveResult | save results to hard disk (always enabled, when genMFun and genSLBlock are set)
'logFile', logfile | write code generation progress to specified logfile
'genMFun' | generate robot specific m-functions
'genSLBlock' | generate real-time capable robot specific Simulink blocks
'genccode' | generate robot specific C-functions and -headers
'mex' | generate robot specific MEX-functions as replacement for the m-functions
'compilemex' | select whether generated MEX-function should be compiled directly after generation

Any option may also be modified individually as optional parameter value pairs.

## Author

Joern Malzahn 2012 RST, Technische Universitaet Dortmund, Germany. http://www.rst.e-technik.tu-dortmund.de

# CodeGenerator.addpath

Adds generated code to search path

cGen.addpath() adds the generated m-functions and block library to the MATLAB function search path.

## Author

Joern Malzahn 2012 RST, Technische Universitaet Dortmund, Germany. http://www.rst.e-technik.tu-dortmund.de

## See also

addpath

# CodeGenerator.genccodecoriolis

Generate C-function for robot inertia matrix

cGen.genccodecoriolis() generates robot-specific C-functions to compute the robot coriolis matrix.

## Notes

- Is called by CodeGenerator.gencoriolis if cGen has active flag genccode or genmex.
- The .c and .h files are generated in the directory specified by the ccodepath property of the CodeGenerator object.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gencoriolis, CodeGenerator.genmexcoriolis

# CodeGenerator.genccodefdyn

Generate C-code for forward dynamics

cGen.genccodeinvdyn() generates a robot-specific C-code to compute the forward dynamics.

## Notes

- Is called by CodeGenerator.genfdyn if cGen has active flag genccode or genmex.
- The .c and .h files are generated in the directory specified by the ccodepath property of the CodeGenerator object.
- The resulting C-function is composed of previously generated C-functions for the inertia matrix, Coriolis matrix, vector of gravitational load and joint friction vector. This function recombines these components to compute the forward dynamics.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genfdyn, CodeGenerator.genccodeinvdyn

# CodeGenerator.genccodefkine

Generate C-code for the forward kinematics

cGen.genccodefkine() generates a robot-specific C-function to compute forward kinematics.

## Notes

- Is called by CodeGenerator.genfkine if cGen has active flag genccode or genmex
- The generated .c and .h files are wirtten to the directory specified in the ccodepath property of the CodeGenerator object.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genfkine, CodeGenerator.genmexfkine

# CodeGenerator.genccodefriction

Generate C-code for the joint friction

cGen.genccodefriction() generates a robot-specific C-function to compute vector of friction torques/forces.

## Notes

- Is called by CodeGenerator.genfriction if cGen has active flag genccode or genmex
- The generated .c and .h files are wirtten to the directory specified in the ccodepath property of the CodeGenerator object.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genfriction, CodeGenerator.genmexfriction

# CodeGenerator.genccodegravload

Generate C-code for the vector of

gravitational load torques/forces

cGen.genccodegravload() generates a robot-specific C-function to compute vector of gravitational load torques/forces.

## Notes

- Is called by CodeGenerator.gengravload if cGen has active flag genccode or genmex
- The generated .c and .h files are wirtten to the directory specified in the ccodepath property of the CodeGenerator object.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gengravload, CodeGenerator.genmexgravload

# CodeGenerator.genccodeinertia

Generate C-function for robot inertia matrix

cGen.genccodeinertia() generates robot-specific C-functions to compute the robot inertia matrix.

## Notes

- Is called by CodeGenerator.geninertia if cGen has active flag genccode or genmex.
- The generated .c and .h files are generated in the directory specified by the ccodepath property of the CodeGenerator object.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninertia, CodeGenerator.genmexinertia

# CodeGenerator.genccodeinvdyn

Generate C-code for inverse dynamics

cGen.genccodeinvdyn() generates a robot-specific C-code to compute the inverse dynamics.

## Notes

- Is called by CodeGenerator.geninvdyn if cGen has active flag genccode or genmex.
- The .c and .h files are generated in the directory specified by the ccodepath property of the CodeGenerator object.
- The resulting C-function is composed of previously generated C-functions for the inertia matrix, coriolis matrix, vector of gravitational load and joint friction vector. This function recombines these components to compute the inverse dynamics.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninvdyn, CodeGenerator.genccodefdyn

# CodeGenerator.genccodejacobian

Generate C-functions for robot jacobians

cGen.genccodejacobian() generates a robot-specific C-function to compute the jacobians with respect to the robot base as well as the end effector.

## Notes

- Is called by CodeGenerator.genjacobian if cGen has active flag genccode or genmex.
- The generated .c and .h files are generated in the directory specified by the ccodepath property of the CodeGenerator object.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genccodefkine, CodeGenerator.genjacobian

# CodeGenerator.gencoriolis

Generate code for Coriolis force

coriolis = cGen.gencoriolis() is a symbolic matrix (NxN) of centrifugal and Coriolis forces/torques.

## Notes

- The Coriolis matrix is stored row by row to avoid memory issues. The generated code recombines these rows to output the full matrix.
- Side effects of execution depends on the cGen flags:

- saveresult: the symbolic expressions are saved to disk in the directory specified by cGen.sympath
- genmfun: ready to use m-functions are generated and provided via a subclass of SerialLink stored in cGen.robjpath
- genslblock: a Simulink block is generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath
- genccode: generates C-functions and -headers in the directory specified by the ccodepath property of the CodeGenerator object.
- mex: generates robot specific MEX-functions as replacement for the m-functions mentioned above. Access is provided by the SerialLink subclass. The MEX files rely on the C code generated before.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninertia, CodeGenerator.genfkine

# CodeGenerator.genfdyn

Generate code for forward dynamics

Iqdd = cGen.genfdyn() is a symbolic vector (1xN) of joint inertial reaction forces/torques.

## Notes

- Side effects of execution depends on the cGen flags:

- saveresult: the symbolic expressions are saved to disk in the directory specified by cGen.sympath
- genmfun: ready to use m-functions are generated and provided via a subclass of SerialLink stored in cGen.robjpath
- genslblock: a Simulink block is generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath
- genccode: generates C-functions and -headers in the directory specified by the ccodepath property of the CodeGenerator object.
- mex: generates robot specific MEX-functions as replacement for the m-functions mentioned above. Access is provided by the SerialLink subclass. The MEX files rely on the C code generated before.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninertia, CodeGenerator.genfkine

# CodeGenerator.genfkine

Generate code for forward kinematics

T = cGen.genfkine() generates a symbolic homogeneous transform matrix (4x4) representing the pose of the robot end-effector in terms of the symbolic joint coordinates q1, q2, ...

[T, allt] = cGen.genfkine() as above but also generates symbolic homogeneous transform matrices (4x4xN) for the poses of the individual robot joints.

## Notes

- Side effects of execution depends on the cGen flags:

- saveresult: the symbolic expressions are saved to disk in the directory specified by cGen.sympath
- genmfun: ready to use m-functions are generated and provided via a subclass of SerialLink stored in cGen.robjpath
- genslblock: a Simulink block is generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath
- genccode: generates C-functions and -headers in the directory specified by the ccodepath property of the CodeGenerator object.
- mex: generates robot specific MEX-functions as replacement for the m-functions mentioned above. Access is provided by the SerialLink subclass. The MEX files rely on the C code generated before.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninvdyn, CodeGenerator.genjacobian

# CodeGenerator.genfriction

Generate code for joint friction

f = cGen.genfriction() is the symbolic vector (1xN) of joint friction forces.

## Notes

- Side effects of execution depends on the cGen flags:

- saveresult: the symbolic expressions are saved to disk in the directory specified by cGen.sympath
- genmfun: ready to use m-functions are generated and provided via a subclass of SerialLink stored in cGen.robjpath
- genslblock: a Simulink block is generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath
- genccode: generates C-functions and -headers in the directory specified by the ccodepath property of the CodeGenerator object.
- mex: generates robot specific MEX-functions as replacement for the m-functions mentioned above. Access is provided by the SerialLink subclass. The MEX files rely on the C code generated before.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninvdyn, CodeGenerator.genfdyn

# CodeGenerator.gengravload

Generate code for gravitational load

g = cGen.gengravload() is a symbolic vector (1xN) of joint load forces/torques due to gravity.

## Notes

- Side effects of execution depends on the cGen flags:

- saveresult: the symbolic expressions are saved to disk in the directory specified by cGen.sympath
- genmfun: ready to use m-functions are generated and provided via a subclass of SerialLink stored in cGen.robjpath
- genslblock: a Simulink block is generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath
- genccode: generates C-functions and -headers in the directory specified by the ccodepath property of the CodeGenerator object.
- mex: generates robot specific MEX-functions as replacement for the m-functions mentioned above. Access is provided by the SerialLink subclass. The MEX files rely on the C code generated before.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator, CodeGenerator.geninvdyn, CodeGenerator.genfdyn

# CodeGenerator.geninertia

Generate code for inertia matrix

i = cGen.geninertia() is the symbolic robot inertia matrix (NxN).

## Notes

- The inertia matrix is stored row by row to avoid memory issues. The generated code recombines these rows to output the full matrix.
- Side effects of execution depends on the cGen flags:

- saveresult: the symbolic expressions are saved to disk in the directory specified by cGen.sympath
- genmfun: ready to use m-functions are generated and provided via a subclass of SerialLink stored in cGen.robjpath
- genslblock: a Simulink block is generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath
- genccode: generates C-functions and -headers in the directory specified by the ccodepath property of the CodeGenerator object.
- mex: generates robot specific MEX-functions as replacement for the m-functions mentioned above. Access is provided by the SerialLink subclass. The MEX files rely on the C code generated before.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninvdyn, CodeGenerator.genfdyn

# CodeGenerator.geninvdyn

Generate code for inverse dynamics

tau = cGen.geninvdyn() is the symbolic vector (1xN) of joint forces/torques.

## Notes

- The inverse dynamics vector is composed of the previously computed inertia matrix coriolis matrix, vector of gravitational load and joint friction for speedup. The generated code recombines these components to output the final vector.
- Side effects of execution depends on the cGen flags:

- saveresult: the symbolic expressions are saved to disk in the directory specified by cGen.sympath
- genmfun: ready to use m-functions are generated and provided via a subclass of SerialLink stored in cGen.robjpath
- genslblock: a Simulink block is generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath
- genccode: generates C-functions and -headers in the directory specified by the ccodepath property of the CodeGenerator object.
- mex: generates robot specific MEX-functions as replacement for the m-functions mentioned above. Access is provided by the SerialLink subclass. The MEX files rely on the C code generated before.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genfdyn, CodeGenerator.genfkine

# CodeGenerator.genjacobian

Generate code for robot Jacobians

j0 = cGen.genjacobian() is the symbolic expression for the Jacobian matrix (6xN) expressed in the base coordinate frame.

[j0, Jn] = cGen.genjacobian() as above but also returns the symbolic expression for the Jacobian matrix (6xN) expressed in the end-effector frame.

## Notes

- Side effects of execution depends on the cGen flags:

- saveresult: the symbolic expressions are saved to disk in the directory specified by cGen.sympath
- genmfun: ready to use m-functions are generated and provided via a subclass of SerialLink stored in cGen.robjpath
- genslblock: a Simulink block is generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath
- genccode: generates C-functions and -headers in the directory specified by the ccodepath property of the CodeGenerator object.
- mex: generates robot specific MEX-functions as replacement for the m-functions mentioned above. Access is provided by the SerialLink subclass. The MEX files rely on the C code generated before.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genfkine

# CodeGenerator.genmexcoriolis

Generate C-MEX-function for robot coriolis matrix

cGen.genmexcoriolis() generates robot-specific MEX-functions to compute robot coriolis matrix.

## Notes

- Is called by CodeGenerator.gencoriolis if cGen has active flag genmex
- The MEX file uses the .c and .h files generated in the directory specified by the ccodepath property of the CodeGenerator object.
- Access to generated functions is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.
- You will need a C compiler to use the generated MEX-functions. See the MATLAB documentation on how to setup the compiler in MATLAB. Nevertheless the basic C-MEX-code as such may be generated without a compiler. In this case switch the cGen flag compilemex to false.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gencoriolis

# CodeGenerator.genmexfdyn

Generate C-MEX-function for forward dynamics

cGen.genmexfdyn() generates a robot-specific MEX-function to compute the forward dynamics.

## Notes

- Is called by CodeGenerator.genfdyn if cGen has active flag genmex
- The MEX file uses the .c and .h files generated in the directory specified by the ccodepath property of the CodeGenerator object.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.
- You will need a C compiler to use the generated MEX-functions. See the MATLAB documentation on how to setup the compiler in MATLAB. Nevertheless the basic C-MEX-code as such may be generated without a compiler. In this case switch the cGen flag compilemex to false.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genfdyn, CodeGenerator.genmexinvdyn

# CodeGenerator.genmexfkine

Generate C-MEX-function for forward kinematics

cGen.genmexfkine() generates a robot-specific MEX-function to compute forward kinematics.

## Notes

- Is called by CodeGenerator.genfkine if cGen has active flag genmex
- The MEX file uses the .c and .h files generated in the directory specified by the ccodepath property of the CodeGenerator object.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.
- You will need a C compiler to use the generated MEX-functions. See the MATLAB documentation on how to setup the compiler in MATLAB. Nevertheless the basic C-MEX-code as such may be generated without a compiler. In this case switch the cGen flag compilemex to false.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genfkine

# CodeGenerator.genmexfriction

Generate C-MEX-function for joint friction

cGen.genmexfriction() generates a robot-specific MEX-function to compute the vector of joint friction.

## Notes

- Is called by CodeGenerator.genfriction if cGen has active flag genmex
- The MEX file uses the .c and .h files generated in the directory specified by the ccodepath property of the CodeGenerator object.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.
- You will need a C compiler to use the generated MEX-functions. See the MATLAB documentation on how to setup the compiler in MATLAB. Nevertheless the basic C-MEX-code as such may be generated without a compiler. In this case switch the cGen flag compilemex to false.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gengravload

# CodeGenerator.genmexgravload

Generate C-MEX-function for gravitational load

cGen.genmexgravload() generates a robot-specific MEX-function to compute gravitation load forces and torques.

## Notes

- Is called by CodeGenerator.gengravload if cGen has active flag genmex
- The MEX file uses the .c and .h files generated in the directory specified by the ccodepath property of the CodeGenerator object.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.
- You will need a C compiler to use the generated MEX-functions. See the MATLAB documentation on how to setup the compiler in MATLAB. Nevertheless the basic C-MEX-code as such may be generated without a compiler. In this case switch the cGen flag compilemex to false.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gengravload

# CodeGenerator.genmexinertia

Generate C-MEX-function for robot inertia matrix

cGen.genmexinertia() generates robot-specific MEX-functions to compute robot inertia matrix.

## Notes

- Is called by CodeGenerator.geninertia if cGen has active flag genmex
- The MEX file uses the .c and .h files generated in the directory specified by the ccodepath property of the CodeGenerator object.
- Access to generated functions is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.
- You will need a C compiler to use the generated MEX-functions. See the MATLAB documentation on how to setup the compiler in MATLAB. Nevertheless the basic C-MEX-code as such may be generated without a compiler. In this case switch the cGen flag compilemex to false.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninertia

# CodeGenerator.genmexinvdyn

Generate C-MEX-function for inverse dynamics

cGen.genmexinvdyn() generates a robot-specific MEX-function to compute the inverse dynamics.

## Notes

- Is called by CodeGenerator.geninvdyn if cGen has active flag genmex.
- The MEX file uses the .c and .h files generated in the directory specified by the ccodepath property of the CodeGenerator object.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.
- You will need a C compiler to use the generated MEX-functions. See the MATLAB documentation on how to setup the compiler in MATLAB. Nevertheless the basic C-MEX-code as such may be generated without a compiler. In this case switch the cGen flag compilemex to false.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gengravload

# CodeGenerator.genmexjacobian

Generate C-MEX-function for the robot Jacobians

cGen.genmexjacobian() generates robot-specific MEX-function to compute the robot Jacobian with respect to the base as well as the end effector frame.

## Notes

- Is called by CodeGenerator.genjacobian if cGen has active flag genmex.
- The MEX file uses the .c and .h files generated in the directory specified by the ccodepath property of the CodeGenerator object.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.
- You will need a C compiler to use the generated MEX-functions. See the MATLAB documentation on how to setup the compiler in MATLAB. Nevertheless the basic C-MEX-code as such may be generated without a compiler. In this case switch the cGen flag compilemex to false.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genjacobian

# CodeGenerator.genmfuncoriolis

Generate M-functions for Coriolis matrix

cGen.genmfuncoriolis() generates a robot-specific M-function to compute the Coriolis matrix.

## Notes

- Is called by CodeGenerator.gencoriolis if cGen has active flag genmfun
- The Coriolis matrix is stored row by row to avoid memory issues.
- The generated M-function recombines the individual M-functions for each row.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gencoriolis, CodeGenerator.geninertia

# CodeGenerator.genmfunfdyn

Generate M-function for forward dynamics

cGen.genmfunfdyn() generates a robot-specific M-function to compute the forward dynamics.

## Notes

- Is called by CodeGenerator.genfdyn if cGen has active flag genmfun
- The generated M-function is composed of previously generated M-functions for the inertia matrix, coriolis matrix, vector of gravitational load and joint friction vector. This function recombines these components to compute the forward dynamics.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninvdyn

# CodeGenerator.genmfunfkine

Generate M-function for forward kinematics

cGen.genmfunfkine() generates a robot-specific M-function to compute forward kinematics.

## Notes

- Is called by CodeGenerator.genfkine if cGen has active flag genmfun
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genjacobian

# CodeGenerator.genmfunfriction

Generate M-function for joint friction

cGen.genmfunfriction() generates a robot-specific M-function to compute joint friction.

## Notes

- Is called only if cGen has active flag genmfun
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gengravload

# CodeGenerator.genmfungravload

Generate M-functions for gravitational load

cGen.genmfungravload() generates a robot-specific M-function to compute gravitation load forces and torques.

## Notes

- Is called by CodeGenerator.gengravload if cGen has active flag genmfun
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninertia

# CodeGenerator.genmfuninertia

Generate M-function for robot inertia matrix

cGen.genmfuninertia() generates a robot-specific M-function to compute robot inertia matrix.

## Notes

- Is called by CodeGenerator.geninertia if cGen has active flag genmfun
- The inertia matrix is stored row by row to avoid memory issues.
- The generated M-function recombines the individual M-functions for each row.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gencoriolis

# CodeGenerator.genmfuninvdyn

Generate M-functions for inverse dynamics

cGen.genmfuninvdyn() generates a robot-specific M-function to compute inverse dynamics.

## Notes

- Is called by CodeGenerator.geninvdyn if cGen has active flag genmfun
- The generated M-function is composed of previously generated M-functions for the inertia matrix, coriolis matrix, vector of gravitational load and joint friction vector. This function recombines these components to compute the inverse dynamics.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninvdyn

# CodeGenerator.genmfunjacobian

Generate M-functions for robot Jacobian

cGen.genmfunjacobian() generates a robot-specific M-function to compute robot Jacobian.

## Notes

- Is called by CodeGenerator.genjacobian, if cGen has active flag genmfun
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gencoriolis

# CodeGenerator.genslblockcoriolis

Generate Simulink block for Coriolis matrix

cGen.genslblockcoriolis() generates a robot-specific Simulink block to compute Coriolis/centripetal matrix.

## Notes

- Is called by CodeGenerator.gencoriolis if cGen has active flag genslblock
- The Coriolis matrix is stored row by row to avoid memory issues.
- The Simulink block recombines the the individual blocks for each row.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.gencoriolis

# CodeGenerator.genslblockfdyn

Generate Simulink block for forward dynamics

cGen.genslblockfdyn() generates a robot-specific Simulink block to compute forward dynamics.

## Notes

- Is called by CodeGenerator.genfdyn if cGen has active flag genslblock
- The generated Simulink block is composed of previously generated blocks for the inertia matrix, coriolis matrix, vector of gravitational load and joint friction vector. The block recombines these components to compute the forward dynamics.
- Access to generated function is provided via subclass of SerialLink whose class definition is stored in cGen.robjpath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genfdyn

# CodeGenerator.genslblockfkine

Generate Simulink block for forward kinematics

cGen.genslblockfkine() generates a robot-specific Simulink block to compute forward kinematics.

## Notes

- Is called by CodeGenerator.genfkine if cGen has active flag genslblock.
- The Simulink blocks are generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath.
- Blocks are created for intermediate transforms T0, T1 etc. as well.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genfkine

# CodeGenerator.genslblockfriction

Generate Simulink block for joint friction

cGen.genslblockfriction() generates a robot-specific Simulink block to compute the joint friction model.

## Notes

- Is called by CodeGenerator.genfriction if cGen has active flag genslblock
- The Simulink blocks are generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genfriction

# CodeGenerator.genslblockgravload

Generate Simulink block for gravitational load

cGen.genslblockgravload() generates a robot-specific Simulink block to compute gravitational load.

## Notes

- Is called by CodeGenerator.gengravload if cGen has active flag genslblock
- The Simulink blocks are generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

See also CodeGenerator.CodeGenerator, CodeGenerator.gengravload

# CodeGenerator.genslblockinertia

Generate Simulink block for inertia matrix

cGen.genslbgenslblockinertia() generates a robot-specific Simulink block to compute robot inertia matrix.

## Notes

- Is called by CodeGenerator.geninertia if cGen has active flag genslblock
- The Inertia matrix is stored row by row to avoid memory issues.
- The Simulink block recombines the the individual blocks for each row.
- The Simulink blocks are generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninertia

# CodeGenerator.genslblockinvdyn

Generate Simulink block for inverse dynamics

cGen.genslblockinvdyn() generates a robot-specific Simulink block to compute inverse dynamics.

## Notes

- Is called by CodeGenerator.geninvdyn if cGen has active flag genslblock
- The generated Simulink block is composed of previously generated blocks for the inertia matrix, coriolis matrix, vector of gravitational load and joint friction vector. The block recombines these components to compute the forward dynamics.
- The Simulink blocks are generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.geninvdyn

# CodeGenerator.genslblockjacobian

Generate Simulink block for robot Jacobians

cGen.genslblockjacobian() generates a robot-specific Simulink block to compute robot Jacobians (world and tool frame).

## Notes

- Is called by CodeGenerator.genjacobian if cGen has active flag genslblock
- The Simulink blocks are generated and stored in a robot specific block library cGen.slib in the directory cGen.basepath.

## Author

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

CodeGenerator.CodeGenerator, CodeGenerator.genjacobian

# CodeGenerator.logmsg

Print CodeGenerator logs.

count = CGen.logmsg( FORMAT, A, ...) is the number of characters written to the CGen.logfile. For the additional arguments see fprintf.

## Note

Matlab ships with a function for writing formatted strings into a text file or to the console (fprintf). The function works with single target identifiers (file, console, string). This function uses the same syntax as for the fprintf function to output log messages to either the Matlab console, a log file or both.

## Authors

Joern Malzahn, (joern.malzahn@tu-dortmund.de)

## See also

multidfprintf, fprintf, sprintf

# CodeGenerator.purge

Cleanup generated files

cGen.purge() deletes all generated files, first displays a question dialog to make sure the user really wants to delete all generated files.

cGen.purge(1) as above but skips the question dialog.

## Author

Joern Malzahn 2012 RST, Technische Universitaet Dortmund, Germany. http://www.rst.e-technik.tu-dortmund.de

# CodeGenerator.rmpath

Removes generated code from search path

cGen.rmpath() removes generated m-functions and block library from the MATLAB function search path.

## Author

Joern Malzahn 2012 RST, Technische Universitaet Dortmund, Germany. http://www.rst.e-technik.tu-dortmund.de

## See also

rmpath

© 1990-2014 Peter Corke.