M-File Help: DHFactor | View code for DHFactor

# DHFactor

Simplify symbolic link transform expressions

f = dhfactor(s) is an object that encodes the kinematic model of a robot provided by a string s that represents a chain of elementary transforms from the robot's base to its tool tip. The chain of elementary rotations and translations is symbolically factored into a sequence of link transforms described by DH parameters.

For example:

    s = 'Rz(q1).Rx(q2).Ty(L1).Rx(q3).Tz(L2)';

indicates a rotation of q1 about the z-axis, then rotation of q2 about the x-axis, translation of L1 about the y-axis, rotation of q3 about the x-axis and translation of L2 along the z-axis.

## Methods

base | the base transform as a Java string
tool | the tool transform as a Java string
command | a command string that will create a SerialLink() object representing the specified kinematics
char | convert to string representation
display | display in human readable form

## Example

    >> s = 'Rz(q1).Rx(q2).Ty(L1).Rx(q3).Tz(L2)';
    >> dh = DHFactor(s);
    >> dh
    DH(q1+90, 0, 0, +90).DH(q2, L1, 0, 0).DH(q3-90, L2, 0, 0).Rz(+90).Rx(-90).Rz(-90)
    >> r = eval( dh.command('myrobot') );

## Notes

- Variables starting with q are assumed to be joint coordinates.
- Variables starting with L are length constants.
- Length constants must be defined in the workspace before executing the last line above.
- Implemented in Java.
- Not all sequences can be converted to DH format, if conversion cannot be achieved an error is generated.

## Reference

- A simple and systematic approach to assigning Denavit-Hartenberg parameters, P.Corke, IEEE Transaction on Robotics, vol. 23, pp. 590-594, June 2007.
- Robotics, Vision & Control, Sec 7.5.2, 7.7.1, Peter Corke, Springer 2011.

## See also

SerialLink

© 1990-2014 Peter Corke.